These functions show how to load the memories for the Hotstate machine. 
You may need to customize this code for different boards.
The parser and parserRL (parser runtime loading) examples 
have all been run on the Xilinx Kria vision starter board.
This application should run on any system based on any of the 
the Zynq Ultrascale+ devices with the exception of the Kria
fan I/O which can be deleted.

Copy the release to the Kria and unzip and run install_hot

These libraries should be compiled by install_hot on the target ARM of the Kria.

These libs have been tested on the Kria only under Ubuntu 22.04

